**REMUS product information 16-2016**

**AUDI TTS Quattro, Coupe & Cabrio, type 8S, 2014=>**

Dear **REMUS** Partner,

We are pleased to inform you that we have completed our next development:

**REMUS resonated middle section or racing section and REMUS L/R sport exhaust system with selectable tail pipes for the**

**AUDI TTS Quattro, Coupe & Cabrio, type 8S, 2014=>**.

It would be a pleasure for us to receive your orders.

Stay tuned!


Your **REMUS** Team



**#70SS: Stainless steel tail pipes Ø 102 mm angled/angled, chromed**

**#70CSS: Carbon tail pipes Ø 102 mm angled/angled, Titanium internals**





|  |  |  |
| --- | --- | --- |
| **Car and engine specification** | | |
| **AUDI TTS Quattro, Coupe & Cabrio, Type 8S, 2014=>**  2.0l TFSI 228 kW (CJX) | | |
| **Part no.** | **Description** | **€ RRP price excl. VAT** |
| **046014 0000** | Stainless steel non-resonated racing middle section, without homologation  Original tube Ø 70 mm / REMUS tube Ø 70 mm | **85,--** |
|  | | |
| **046014 0400** | Stainless steel resonated middle section, with EEC homologation  Original tube Ø 70 mm / REMUS tube Ø 70 mm | **240,--** |
|  | | |
| **045114 0000** | Stainless steel connection tube for mounting the sport exhaust | **84,--** |
| **046014 1500** | Stainless steel sport exhaust centered L/R system (without tail pipes), with 2 integrated electrical valves, with EEC homologation  Original tube Ø 70 mm / REMUS tube Ø 70 mm | **710,--** |
| **choose from following tail pipe package:** | | |
| **0046 70SS** | Stainless steel tail pipe set L/R consisting of 4 tail pipes Ø 102 mm angled/angled, chromed, with adjustable spherical clamp connection | **320,--** |
| **0046 70CSS** | Stainless steel tail pipe set L/R consisting of 4 Carbon tail pipe Ø 102 mm angled/angled, Titanium internals, with adjustable spherical clamp connection | **740,--** |
|  | | |
| **INFOBOX:**   * Connection tube, sport exhaust and tail pipe set only fit as a complete system! * No rear skirt modifications required! * Axle-back-system: 045114 0000 + 046014 1500 + tail pipe set. The original exhaust will need to be cut at the manufacturer marked cutting point! * Cat-back-system: 046014 0000 alternatively 046014 0400 and 045114 0000 + 046014 1500 + tail pipe set. No vehicle modifications required! | | |

****



**Under** [**http://www.remus.eu/powerizer/**](http://www.remus.eu/powerizer/) **and** [**http://www.remus.eu/remusresponder**](http://www.remus.eu/remusresponder) **you will find the entire product range, prices and installation instructions.**

|  |
| --- |
| **REMUS Powerizer: More power, more economy and more fun.**   * Up to 25 % more power * Up to 20 % more torque * Up to 1l/100 km fuel saving * Fully adjustable power increase * Simple DIY installation (Plug & Play)   REMUS POWERIZER: The performance figures represent the maximum achievable values. The actual performance output depends on the original tolerances of each engine. REMUS delivers the POWERIZER with the best possible setting for your vehicle type. You can adjust the performance according to your requirements as per the POWERIZER instructions  **Legal references**  *1. Completion and registration of chip tuning in the car documents*  Due to chip tuning, the operating license of the vehicle will terminate if the installation and registration of the POWERIZER is not carried out or immediately reported to an official approved testing facility. Please consider that driving a vehicle without the required operating license will cause legal penalties.  *2. Vehicle insurance must be informed upon installing a POWERIZER*  The installation of the POWERIZER can have influence on the insurance policy of your vehicle. You must inform the insurance company if you install a POWERIZER in your vehicle.  *3. Effect of chip tuning on warranty and guarantee claims*  a) When installing a POWERIZER, you will lose all guarantee claims regarding the engine against the vehicle manufacturer.  b) Installing a POWERIZER, can have influence on warranty claims against the seller of the vehicle.  c) REMUS excludes any claims regarding compensation for damages on the engine and drivetrain. |





**Under** [**http://www.remus.eu/powerizer/**](http://www.remus.eu/powerizer/) **and** [**http://www.remus.eu/remusresponder**](http://www.remus.eu/remusresponder) **you will find the entire product range, prices and installation instructions.**

|  |
| --- |
| **REMUS RESPONDER:**  **Improved throttle response, more dynamic!**  The REMUS Responder improves throttle response by means of modifying the accelerator pedal output signal. No more throttle delay and reduced lag during automatic shifting makes driving with the REMUS Responder more fun. The Responder attaches between the OEM pedal sensor and the OEM connector, ready to use in seconds due to plug & play technology. Sophisticated adjustable programming profiles can lead to improved fuel consumption and more efficiency. The 4 individual user selectable and adjustable performance settings allow drivers to select according to their own preferences.  The REMUS Responder totally eliminates the delay in modern electronic accelerator pedals! |

